
1. Copy only "cvrcp.v1.5.15-web.pk" file without any folder to an empty USB thumb drive. (*Note: USB thumb drive file system needs to be FAT32)
2. Turn on RCP-PLUS.
3. Plug USB thumb drive to RCP-PLUS USB port, the update will start automatically.
4. Once you see the message "Update success, Going to Reboot", you can remove USB thumb drive.
5. After rebooting, confirm the version number at lower right corner of the screen.